******************************************************************

Local Setup for Diagnostic (LSD) for Windows 98SE, Me, 2000, XP, 2003

******************************************************************

1. About LSD
This LSD software utility provides one easy way to set up those
functions following below.
The LSD supports Windows 98SE, Me, 2000, 2003 and XP.
For LSD operation, the USB 1.1/2.0 cable needs to be connected to the
machine. The USB Port allows you to operate those operations by
this software.
(1) Registration and edition of One-Touch dial, Speed dial and
    Group dial.
(2) Indication of machine's counter or Status.
(3) Alteration of machine's setting.


2. Installing the LSD
Before installing LSD, please check your PC that TWAIN Driver is
installed. For installing the TWAIN Driver, please see
Readme(TWAIN).txt, or the installing manual of TWAIN Driver.
(1) Readme(TWAIN).txt : There's the file in "Driver" folder of
    machine's accessories Driver CD.
(2) TWAIN Driver Installing manual : There's the file in "Manual"
    folder of machine's accessories Driver CD.

2.1 Windows XP/2000
For LSD set up, administrator ID need to be input. Please start
the installing by following procedure after you log in as the
administrator.
(1) For Windows running, insert the CD-ROM into your computer's
    CD-ROM drive.
(2) Execute LSDSetup.exe.
(3) Select the model and language that you handle, then press OK button.
(4) As you continue the operation of the following instruction,
    the LSD installing is completed.

2.2 Windows Me/98SE
Please execute the installing by following procedure.
(1) For Windows running, insert the CD-ROM into your computer's
    CD-ROM drive.
(2) Execute LSDSetup.exe.
(3) Select the model and language that you handle, then press OK button.
(4) As you continue the operation of the following instruction,
    the LSD installing is completed.


3. How to use LSD
Please make sure that your machine's Main Power is ON.
Please start from Windows [Start] -> [Program].
When LSD shows no reaction, please make sure that the USB port is
correctly connected, or check the machine's display whether it
has error message or not.
During the machine is working or operating LSD cannot be connected.
And while LSD is connected, the operation cannot be performed from
the machine's panel.


4. Release note
* In the operation Machine-Utility Setting-Rx Operation-Memory Rx,
  Password and Time are not be changed with the setting is ON->ON.
  When you change Password and Time, please set it OFF first,
  then set it ON.
  (The setting needs to be uploaded to the machine.)
* "Upload" from LSD overwrites LSD's data on all of the machine's
  data. Please "Download" and "Save" first, if you want to keep
  the current machine's data.
* In Program Dial, both "edition in LSD" and "Upload to the
  machine" cannot be performed.
* After data is uploaded from LSD to the machine, be sure to turn
  machine's main power OFF and ON.
* If setting "Auto Shut Off" invalid in [Administrator mode],
  it might not be change the setting/time of "Auto Shut Off"
  in [Machine Setting]. In this case, please re-open the window
  of Utility Setting.


Microsoft and Windows are registered trademarks of Microsoft
Corporation.
